~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
P A T C H M A N   M U S I C
1600 Saint Charles Avenue
Lakewood, OH 44107

Phone:
216-221-8282

E-mail:
matt@patchmanmusic.com

Web Site:
http://www.patchmanmusic.com
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Thank you for purchasing PATCHMAN MUSIC Pro Patches Volume 1 for the Korg M1. This unique bank of 100 Programs and 100 Combinations was specifically designed to be used with a wind controller such as the Yamaha WX5, WX7, WX11, WindJamm'r, MIDI EVI, Akai EVI, EWI, or Synthophone. Keyboardists can also enjoy these sounds by using a BC1, BC2, or BC3 breath controller plugged directly into a keyboard equipped with a breath controller input or into a device such as the Midi Solutions Breath Controller Box (www.midisolutions.com) or an Anatek Wind Machine (out of production). The names of all of these wind controller Programs and Combinations begin with a "@" for easy identification.

Before you begin you might want to print out these instructions for easier access while you are going through the following steps.


==============================================
Prepare The M1/r To Receive The New Sounds
==============================================
Before you can transmit these new sounds to the M1/r you need to prepare it to receive system exclusive data. To do this...

On the M1/r, set the Global Midi Channel to 1...
1.) Push "GLOBAL"
2.) Push "PAGE+" 10 times until the display reads "MIDI GLOBAL" 
3.) Push the "C" button
4.) Push the "UP" or "DOWN" button until the display reads "CH= 1"

Next, make sure Sysex reception is Enabled for both Programs and Combis...
1.) Push "GLOBAL"
2.) Push "PAGE+" once until the display reads "MIDI FILTERING" 
3.) Push the "H" button
4.) Push the "UP" button until the display reads "EXCL:ENA"

Next, make sure Aftertouch reception is enabled...
1.) Push the "C" button
2.) Push the "UP" button until the display reads "AFTT:ENA"

Next, make sure Control Change reception is enabled...
1.) Push the "F" button
2.) Push the "UP" button until the display reads "CNTL:ENA"

Next, turn off PROGRAM MEMORY PROTECT...
1.) Push "PAGE+" once. The display should read "PROGRAM MEMORY PROTECT" 
2.) Push the "C" button
3.) Push the "DOWN" button until the display reads "Internal:OFF"

Next, turn off COMBINATION MEMORY PROTECT...
1.) Push "PAGE+" once again. The display should read "COMBINATION MEMORY PROTECT" 
2.) Push the "C" button
3.) Push the "DOWN" button until the display reads "Internal:OFF"

Set MEMORY ALLOCATION to (100PROG/100COMBI/440SEQ)...
1.) Push "PAGE+" 2 times until display reads "Memory Allocation" 
2.) Push the "A" button
3.) Push the "DOWN" button until the display reads "(100PROG/100COMBI/440SEQ)"
4.) Push the "G" button twice to execute this change.

Exit the Global page by pushing the "PROG" or "COMBI" button.


=======================================
 WARNING
=======================================
You may want to save the your current "I" Bank Programs and Combinations because they will be erased once you load this new bank.


=======================================
Using The .SYX File with a PC
=======================================
The .SYX file format is a widely used, standard format for transferring soundbank files. SYX files can be used with a variety of shareware utilities as well as many PC sequencers such as Cakewalk. If you are using Cakewalk simply select "Sysx" under the View menu, select "Load Bank", load in the .SYX file, then select "Send" to send the file. Even the Cakewalk demo is able to transfer .SYX files. A link to several downloadable PC utilities that work with Sysex files is available at:
http://www.patchmanmusic.com/Sysex_Utilities.html


=======================================
Using the Standard MIDIFile (.MID) Format
=======================================
The Standard MIDIfile format consists of a Standard MIDIfile which when played through a MIDI sequencer will load the new sounds into the M1/r. Most sequencers allow you to import or open Standard MIDIfiles. Please consult your sequencer manual if you are not sure how to do this. Once the file has been opened and you have prepared the M1/r, simply "play" the sequence to transmit the sounds into the M1/r. Allow approximately 10 seconds for the full file to transfer.


=======================================
Using The Mac Self Loader Utility
=======================================
To use the Macintosh Self Loader (.SYX) format you will need to use the "Bulk Sysex Utility" application in order to load these sounds into the M1/r. This MIDI application will work with most Macintosh MIDI interfaces. Double click on the "Bulk Sysex Utility" application found on this disk. Push the "Continue" button. Under the MIDI menu, select the appropriate "Port" and "Clock" settings. Select "Bulk sysex" from the MIDI menu. Push the "Open" button. Open the "PMM1V1.SYX" file. Turn on "Slow Transmit" by clicking on the "Slow Transmit" checkbox. Push the "Transmit" button. This file takes approximately 15 seconds to fully transmit. Give it enough time to finish. Quit the "Bulk Sysex Utility" application. M1/r Volume 1 should now be in bank "I" of the M1/r. A link to several other downloadable Mac utilities that work with Sysex files is available at:
http://www.patchmanmusic.com/Sysex_Utilities.html


=======================================
Setting Up Your Wind Controller
=======================================
Since the M1/r is not capable of responding to breath controller data, all of these Programs and Combinations have been programmed to respond to AFTERTOUCH data. Make sure your wind controller is set to transmit AFTERTOUCH data not breath controller data. WX5, WX11, and WindJamm'r users will need to use a mapper (such as Anatek's Pocket Mapper or Wind Machine) to remap breath controller data into aftertouch data. For optimum playing response we recommend not transmitting velocity, breath controller, modulation, or volume data. Velocity parameters have been turned off in these patches anyway. Akai EWI/EVI players please note these sounds are set up such that you should not use the EXT IN on the EWV. Simply use the audio out from the M1/r.


=======================================
If There Are Problems
=======================================
* Make sure the MIDI data is actually being received by the M1.
* Make sure the MIDI data is going out the correct serial port (modem or printer).
* Make sure the M1 has been properly prepared. (See above).
* Make sure you've allowed enough time for the entire transmission to complete.
* If you are hearing the correct notes but very faintly then your wind controller is not transmitting aftertouch data. To correct this please see above.


=======================================
PATCHMAN MUSIC 
M1/r VOLUME 1
PROGRAMS
=======================================
00 @Tenor Sax
01 @Dbl. Reed
02 @Flute
03 @Pan Flute
04 @Clarinet
05 @BassClrnt
06 @Bottles
07 @Voices
08 @Choir
09 @Choir Oct
10 @VoiceWave
11 @Saxy
12 @ReedLayer
13 @Pan-Lyle
14 @Shakupan
15 @PanShak
16 @Shakuhat1
17 @Shakuhat2
18 @Lyle Pan
19 @Bellfazer
20 @HarmonTpt
21 @Trumpet
22 @TubaFlug
23 @Brass 1
24 @Brass 2
25 @Brass 3
26 @Brs2/Tpt
27 @Brs1/Tpt
28 @Brs/M.Tpt
29 @EVI Trmpt
30 @Pulse Tpt
31 @FutureBrs
32 @Tpt/MtTpt
33 @SynBrass
34 @Concertin
35 @Belltonal
36 @25% Pulse
37 @Fazer
38 @Vox Lead
39 @MeloBrass
40 @Strings
41 @D.Guitar1
42 @D.Guitar2
43 @D.Guitar3
44 @EML Pulse
45 @4thSquare
46 @5thSquare
47 @8vaSquare
48 @4th Saw
49 @5th Saw
50 @8va Saw
51 @Matrix 1
52 @Matrix 2
53 @JunoBrass
54 @Pulsar
55 @Snazzy
56 @JazzBop
57 @MiltonBB
58 @Lyle OBx
59 @MelloTrox
60 @SaxoVox
61 @Sax&Miles
62 @Sax&Pan
63 @Trmpt&Pan
64 @ProphetBr
65 @K4 Lead
66 @BrightBrs
67 @Orient 5
68 @AmbPanFl.
69 @Thailand
70 @Manchu
71 @Mandolin1
72 @Mandolin2
73 @Mandolin3
74 @Polestrum
75 @PanTrem
76 @BambooTr
77 @Koto Trem
78 @Windbells
79 @Pole
80 @Pop
81 @Wire
82 @Wire Unis
83 @Wire 8va
84 @Scotch
85 @D110 Lead
86 @Metheny 1
87 @Metheny 2
88 @Chick Ld.
89 @BreckerLd
90 @Vibey
91 @Bellhorn
92 @Vibes
93 @Vibeology
94 @Basswave
95 @Bassey
96 @FretlssBs
97 @AcoustBs
98 @SynthBs1
99 @SynthBs2


=======================================
PATCHMAN MUSIC
M1/r VOLUME 1
COMBINATIONS
=======================================
00 @OctTenors
01 @Tenor/Flt
02 @Ten/PanFl
03 @Ten/Clarn
04 @Ten/BsCla
05 @Ten/LylPn
06 @Ten/MTpt
07 @Shakuhat
08 @Shakusax
09 @ShakuBell
10 @Paninet
11 @SoftPipe
12 @Bellvox
13 @Wide Lead
14 @Prophet
15 @Duneflute
16 @BottlePan
17 @Reed Pan
18 @Pan Lyr
19 @Panfaze
20 @Tpt Sectn
21 @Jazz Tpts
22 @4 M. Tpts
23 @MTpt/Shak
24 @MTpt/Pan
25 @MTpt/SyBr
26 @2 Trmpts
27 @Tpt+Methn
28 @VoxTpt
29 @TptsSaxes
30 @LowSaxes
31 @BreckyLd1
32 @BreckyLd2
33 @BreckyLd3
34 @Chick Ld.
35 @Metheny 1
36 @Metheny 2
37 @Metheny 3
38 @God Vox
39 @Hornvox
40 @StringSec
41 @OrchStrng
42 @Strng/Pan
43 @Strng/Chr
44 @Piper
45 @HarmoVox
46 @--OBx--
47 @Xpander1
48 @Xpander2
49 @Xpander3
50 @PulseWave
51 @UncleMilt
52 @Ten-fore
53 @Fanfare
54 @K4 Lead
55 @K4 Pan Fl
56 @2 Shakus
57 @Lyle OBx
58 @Power Ld
59 @Jammer!
60 @8 Tenors!
61 @Hammondy
62 @Jazz Vibe
63 @Rotation
64 @BreckyBel
65 @MelloBell
66 @Osaki
67 @Hiroshima
68 @Mandolins
69 @Godfather
70 @DistGuit1
71 @DistGuit2
72 @DistGt5th
73 @Bass/Vibe
74 @Bassohol
75 @Bassvivox
76 @SynBass1
77 @SynBass2
78 @Fretless
79 @Fretls/Vb
80 @Breckery1
81 @4 Tpt-sus
82 @4 Sax-sus
83 @WindEnSus
84 @TenorSect
85 @Vibechord
86 @BreckyChd
87 @Turkish
88 @KingsHorn
89 @4th Chick
90 @Regalhorn
91 @Square4-5
92 @TenorSect
93 @DarkChord
94 @WideLead
95 @VoxBox
96 @EVITpt4th
97 @Ishmael
98 @Stringvox
99 @Ben Hur!!

These patches are Copyright ©1994, 2002 PATCHMAN MUSIC All Rights Reserved. Duplication for purposes other than backing up is strictly prohibited. This software is licensed to one user only and cannot be sold, transferred, or used by any other party. To read the complete license pertaining to this software, please visit:
http://www.patchmanmusic.com/License_Agreement.html


=======================================
Lifetime Guarantee
=======================================
Because we offer software products we cannot offer refunds. All software is guaranteed to be free from defects for the life of the software. If you ever encounter a defect simply return the defective software to us for a free replacement. This guarantee is valid only within the United States for original owners. Foreign orders must include $10 to cover the cost of shipping and handling. To help avoid problems, always make a backup and keep it in a safe place.


=======================================
About PATCHMAN MUSIC
=======================================
PATCHMAN MUSIC has been creating studio quality sounds for pros since 1985.

Keyboard controlled Pro Patches are available for the CZ Series, D-5, D-10, D-20, D-110, DS-1, DX7, DX7II, DX7II-FD, DX21, DX27, DX27s, DX100, ESQ-1, ESQ-m, EX-800, JV-80, JV-90, JV-880, JV-1010, JV-1080, JV-2080 & compatibles, K2000, K2500, K2600 & compatibles, Poly-800, Poly-800II, S5000, S6000, S-550, S-330, SampleCell II, SE-1, Soft SampleCell, SQ-80, SY77, SY99, TG77, TX802, TX81Z, Unity, W-30, XP-30, XP-50, XP-60, and XP-80.

Wind controller/breath controller soundbanks are available for the 05R/W, DS-1, DX7, DX7II, DX7II-FD, EWI3000m, EWI3020m, EWI3030m, EWV2000, ESQ-1, ESQ-m, EX5, EX5R, JV-1010, JV-1080, JV-2080 & compatibles, K2000, K2500, K2600 & compatibles, Matrix-1000, Matrix-6, Matrix-6r, M1, M1R, M3R, MU100R, MU128R, NanoSynth, QS6, QS6.1, QS7, QS7.1, QS8, QS8.1, QSR, QuadraSynth Plus Piano, S4+, SY55, SY77, SY99, T1, T2, T3, TG55, TG77, TX802, TX81Z, Unity, VL1, VL1-m, VL70-m, WT11, X5DR, XP-30, XP-50, XP-60, XP-80, and Z1. These soundbanks were designed specifically to be used with a wind controller or breath controller.

"Let us give your synth a whole new identity!"


=======================================
Wind Controllers Online!
=======================================
Here are some wind controller areas you will want to check out:

YAHOO WIND CONTROLLER GROUP:
Homepage: http://groups.yahoo.com/group/windcontroller/
To Subscribe: windcontroller-subscribe@yahoogroups.com
To Unsubscribe: windcontroller-unsubscribe@yahoogroups.com

THE WIND LIST:
A mailing list dedicated to the discussion of wind controllers, breath controllers and their use. To subscribe to the list, send an email message to "LISTSERV@morgan.ucs.mun.ca" with "subscribe wind <your-name-here>" as the body of the message. Once you are subscribed to the windlist mailing list, you will receive discussions as emails. You can contribute a message to the windlist or ask a question by sending the email message to "WIND@morgan.ucs.mun.ca".

The IWSA (International Wind Synth Association):
http://windsynth.org

USED WIND CONTROLLER GEAR:
http://www.patchmanmusic.com/UsedGear.html

WIND CONTROLLER MUSIC:
mp3.com/stations/wind_controller_music

WIND CONTROLLER LINKS:
http://www.patchmanmusic.com/windControllersOnline.html

-----------------------
updated 5/30/02
